**CHEMICAL TREATMENT (Dichlor)**

**YOUR FILLED SPA MUST BE SUPERVISED AT ALL TIMES WHEN THE LID IS UNLOCKED OR OPEN**

**FRESH WATER STARTUP (Town supply or rain water)**

1. Dissolve 2 caps full of HARDNESS INCREASE in a bucket of warm water and add to spa with pump running. Allow ½ hour to pass before next step.

2. Slowly add 1 cup (250gm) of ALKALINITY INCREASE directly into spa water with pump running. Allow ½

hour to pass before next step.

3. Using a new TEST STRIP, check the pH of the spa water (refer to instructions on test strip container).

If pH is in the OK range, proceed to step 4.

If pH is above the OK range (7.2-7.6), add 1 teaspoon of PH DECREASE directly into spa water with

pump running.

After 10 minutes, re-check the pH of the spa water using a new TEST STRIP and if it is still high, repeat

above step using PH DECREASE until it is in the OK range.

**NB: If PH increase has been used allow 1 hour of pump running time before next step.**

4. Add 2 teaspoons of DICHLOR directly into spa water with pump running and leave spa lid off for 15

minutes. Do not use spa for 2 hours after this treatment.

**DAILY USE (You may skip this step if an Ozone unit is fitted to your spa)**

1. After using the spa, add 1 teaspoon of DICHLOR directly into spa water with pump running and leave

spa lid off for 5 minutes. Do not use spa for 1 hour after this treatment.

**WEEKLY**

1. Test pH & Alkalinity using a new TEST STRIP. If necessary, adjust with chemical.

2. Shock dose by adding 2 teaspoons of DICHLOR directly into spa water with pump running and leave spa

lid off for 15 minutes. Do not use spa for 2 hours after this treatment.

**2-4 WEEKLY**

1. Degrease the Filter Cartridge using the CARTRIDGE CLEANER (refer to instructions on the container).

(This can be purchased from your local spa / pool shop)

**8-10 WEEKS**

Change water every 8-10 weeks or when TDS (total dissolved solids) reaches 1000ppm

(Water samples can be tested by your local spa / pool shop)

**HIGH USAGE/CLOUDY WATER**

If an unusually high usage of the spa occurs in a day, or the water has suddenly turned cloudy, it may be

necessary to follow up with an additional Shock dose by adding 2-3 teaspoons of DICHLOR directly into spa water with pump running and leave spa lid off for 15 minutes. Do not use spa for 2 hours after this treatment.